[target.'cfg(all(target_arch = "arm", target_os = "none"))']
# uncomment ONE of these three option to make `cargo run` start a GDB session
# which option to pick depends on your system
# You can also replace openocd.gdb by jlink.gdb when using a J-Link.
# runner = "arm-none-eabi-gdb -q -x openocd.gdb"
# runner = "gdb-multiarch -q -x openocd.gdb"
# runner = "gdb -q -x openocd.gdb"
runner = "probe-rs run --chip STM32F303VCTx"

rustflags = [
  "-C", "linker=flip-link",
  # LLD (shipped with the Rust toolchain) is used as the default linker
  "-C", "link-arg=-Tlink.x",
  "-C", "link-arg=-Tdefmt.x",

  # This is needed if your flash or ram addresses are not aligned to 0x10000 in memory.x
  # See https://github.com/rust-embedded/cortex-m-quickstart/pull/95
  "-C", "link-arg=--nmagic",

  # if you run into problems with LLD switch to the GNU linker by commenting out
  # this line
  # "-C", "linker=arm-none-eabi-ld",

  # if you need to link to pre-compiled C libraries provided by a C toolchain
  # use GCC as the linker by commenting out both lines above and then
  # uncommenting the three lines below
  # "-C", "linker=arm-none-eabi-gcc",
  # "-C", "link-arg=-Wl,-Tlink.x",
  # "-C", "link-arg=-nostartfiles",
]

[build]
# comment out the following line if you intend to run unit tests on host machine
target = "thumbv7em-none-eabihf" # Cortex-M4F and Cortex-M7F (with FPU)

[env]
DEFMT_LOG = "info"
